

**Installation Guide of**

**USB to UART chip inf driver**

**Install inf driver in Windows**:   
1. Right click on “silabser.inf” file, then select “Install”.



2. Click “Yes” item.



3. Then USB to UART chip inf driver installed successfully.

一張含有 文字, 螢幕擷取畫面, 軟體, 電腦圖示 的圖片


AI 產生的內容可能不正確。

4. Click "SilabSer\_Order\_Patch20240801.reg" to assign COM port.

一張含有 文字, 螢幕擷取畫面, 軟體, 陳列 的圖片

AI 產生的內容可能不正確。

5. Click “Yes” item.




6. Click “Yes” item.

一張含有 文字, 螢幕擷取畫面, 陳列, 軟體 的圖片

AI 產生的內容可能不正確。

7. Successfully added to the registry, to reboot system to active the change.



I**nstall inf driver in Windows command line**:


1. Open a command prompt with Administrator privilege.

一張含有 文字, 螢幕擷取畫面, 電腦, 軟體 的圖片

AI 產生的內容可能不正確。

2. A - Change to path to the “silabser.inf” located folder.

B - run “pnputil /add-driver silabser.inf /install” to install inf driver




3. Then USB to UART chip inf driver installed successfully.

一張含有 文字, 電子產品, 螢幕擷取畫面, 電腦 的圖片

AI 產生的內容可能不正確。

4. run “regedit.exe /s SilabSer\_Order\_Patch20240801.reg” to assign COM port.



5. Successfully added to the registry, to reboot system to active the change.